# Settings for AUSTAL
#
# history: 
#
# 2021-08-05 uj  information on rated odorants added
#
#############################################################################
#                                                                           #
# Diese Datei darf nicht verändert werden, es sei denn, Sie wissen genau,   #
# was Sie tun.                                                              #
#                                                                           #
# Do not modify this file unless you know exactly what you are doing.       #
#                                                                           #
#############################################################################

[.system]
# deposition parameters for 5 aerosol groups:
VdVec   0.001  0.010  0.050  0.200  0.070        # m/s
VsVec   0.000  0.000  0.040  0.150  0.060        # m/s
WfVec   3.0e-5 1.5e-4 4.4e-4 4.4e-4 4.4e-4       # 1/s
WeVec   0.8    0.8    0.8    0.8    0.8          # 1

[.astl]
# standard species properties:
grps "0-0"      # aerosol groups
unit "g"        # unit of emission
fc   1.0        # factor for concentration
uc  "g/m3"      # unit of concentration
ry   1.0        # reference value (yearly)
dy  -1          # number of decimals (yearly)
nd  -1          # number exceedances (daily)
rd   0.0        # reference value (daily)
dd  -1          # number of decimals (daily)
nh  -1          # number exceedances (hourly)
rh   0.0        # reference value (hourly)
dh  -1          # number of decimals (hourly)
                # deposition settings
vd   0.0        # deposition velocity (m/s)
wf   0.0        # washout factor Lambda (1/s)
we   1.0        # washout exponent Kappa
fn  86400       # factor for deposition
un  "g/(m2*d)"  # unit of deposition
rn   0.0        # reference value for deposition
dn  -1          # number of decimals for deposition
# conversion times NO->NO2
NOxTimes     2.9  2.5  1.9  1.3   0.9   0.3 # h
# assessment threshold for odor hours
OdorThreshold  0.25                         # OU/m3

###################### gaeous substances #######################

[SO2]
grps  "0-0"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
fn 3.1536e8     # factor for deposition
un "kg/(ha*a)"  # unit of deposition
ry       50     # reference value (yearly)
dy        1     # number of decimals (yearly)
nd        3     # number exceedances (daily)
rd    125.0     # reference value (daily)
dd        0     # number of decimals (daily)
nh       24     # number exceedances (hourly)
rh    350.0     # reference value (hourly)
dh        0     # number of decimals (hourly)
                # deposition settings
vd    0.010     # deposition velocity (m/s)
wf   2.0e-5     # washout factor Lambda (1/s)
we      1.0     # washout exponent Kappa
rn      1.0     # reference value for deposition
dn        4     # number of decimals for deposition

[NOX]
grps  "0-0"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
ry     30.0     # reference value (yearly)
dy        1     # number of decimals (yearly)

[NO2]
grps  "0-0"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
fn 3.1536e8     # factor for deposition
un "kg/(ha*a)"  # unit of deposition
ry     40.0     # reference value (yearly)
dy        1     # number of decimals (yearly)
nh       18     # number exceedances (hourly)
rh    200.0     # reference value (hourly)
dh        0     # number of decimals (hourly)
                # deposition settings
vd    0.003     # deposition velocity (m/s)
wf   1.0e-7     # washout factor Lambda (1/s)
we      1.0     # washout exponent Kappa
rn      1.0     # reference value for deposition
dn        4     # number of decimals for deposition

[NO]
grps  "0-0"     # aerosol groups
unit    "g"     # unit of emission
fn 3.1536e8     # factor for deposition
un  "kg/(ha*a)" # unit of deposition
ry      0.0     # reference value (yearly)
                # deposition settings
vd   0.0005     # deposition velocity (m/s)
rn      1.0     # reference value for deposition
dn        4     # number of decimals for deposition

[NH3]
grps  "0-0"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
fn 3.1536e8     # factor for deposition
un  "kg/(ha*a)" # unit of deposition
ry      3.0     # reference value (yearly)
dy        2     # number of decimals (yearly)
                # deposition settings
vd    0.010     # deposition velocity (m/s)
wf   1.2e-4     # washout factor Lambda (1/s)
we      0.6     # washout exponent Kappa
rn      1.0     # reference value for deposition
dn        4     # number of decimals for deposition

[HG0]
grps  "0-0"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
ry      0.0     # reference value (yearly)
                # deposition settings
vd   0.0003     # deposition velocity (m/s)
fn  8.64e10     # factor for deposition
un  "ug/(m2*d)" # unit of deposition
rn      1.0     # reference value for deposition
dn        3     # number of decimals for deposition

[BZL]
grps  "0-0"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
ry      5.0     # reference value (yearly)
dy        2     # number of decimals (yearly)

[F]
grps  "0-0"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
ry      0.4     # reference value (yearly)
dy        3     # number of decimals (yearly)

[TCE]
grps  "0-0"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
ry     10.0     # reference value (yearly)
dy        2     # number of decimals (yearly)

##################### gaeous/pm substances #####################

[PM]
grps  "1-5"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
fn    86400     # factor for deposition
un  "g/(m2*d)"  # unit of deposition
ry     40.0     # reference value (yearly)
dy        1     # number of decimals (yearly)
nd       35     # number exceedances (daily)
rd     50.0     # reference value (daily)
dd        1     # number of decimals (daily)
rn     0.35     # reference value for deposition
dn        4     # number of decimals for deposition

[PM25]
grps  "1-1"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
ry     25.0     # reference value (yearly)
dy        1     # number of decimals (yearly)

[PB]
grps  "1-5"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
fn  8.64e10     # factor for deposition
un  "ug/(m2*d)" # unit of deposition
ry      0.5     # reference value (yearly)
dy        3     # number of decimals (yearly)
rn    100.0     # reference value for deposition
dn        1     # number of decimals for deposition

[AS]
grps  "1-5"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
fn  8.64e10     # factor for deposition
un  "ug/(m2*d)" # unit of deposition
ry      0.0     # reference value (yearly)
rn      4.0     # reference value for deposition
dn        2     # number of decimals for deposition

[CD]
grps  "1-5"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
fn  8.64e10     # factor for deposition
un  "ug/(m2*d)" # unit of deposition
ry     0.02     # reference value (yearly)
dy        4     # number of decimals (yearly)
rn      2.0     # reference value for deposition
dn        2     # number of decimals for deposition

[NI]
grps  "1-5"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
fn  8.64e10     # factor for deposition
un  "ug/(m2*d)" # unit of deposition
ry      0.0     # reference value (yearly)
rn     15.0     # reference value for deposition
dn        2     # number of decimals for deposition

[HG]
grps  "0-5"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
fn  8.64e10     # factor for deposition
un  "ug/(m2*d)" # unit of deposition
ry      0.0     # reference value (yearly)
rn      1.0     # reference value for deposition
dn        3     # number of decimals for deposition
                # deposition settings for gaseous component
vd    0.005     # deposition velocity (m/s)
wf   1.0e-4     # washout factor Lambda (1/s)
we      0.7     # washout exponent Kappa

[TL]
grps  "1-5"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
fn  8.64e10     # factor for deposition
un  "ug/(m2*d)" # unit of deposition
ry      0.0     # reference value (yearly)
rn      2.0     # reference value for deposition
dn        2     # number of decimals for deposition

[BAP]
grps  "1-5"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e6     # factor for concentration
uc  "ug/m3"     # unit of concentration
fn  8.64e10     # factor for deposition
un  "ug/(m2*d)" # unit of deposition
ry      0.0     # reference value (yearly)
rn      0.5     # reference value for deposition
dn        3     # number of decimals for deposition

[DX]
grps  "1-5"     # aerosol groups
unit    "g"     # unit of emission
fc     1.e12    # factor for concentration
uc  "pg/m3"     # unit of concentration
fn  8.64e16     # factor for deposition
un  "pg/(m2*d)" # unit of deposition
ry      0.0     # reference value (yearly)
rn        9     # reference value for deposition
dn        2     # number of decimals for deposition

[BAE]
grps  "1-5"     # aerosol groups
unit    "1"     # unit of emission
fc        1     # factor for concentration
uc   "1/m3"     # unit of concentration
fn        1     # factor for deposition
un  "1/(m2*s)"  # unit of deposition
ry      1.0     # reference value (yearly)
dy       -1     # number of decimals (yearly)
rn     0.01     # reference value for deposition
dn       -1     # number of decimals for deposition

[XX]
grps  "0-5"     # aerosol groups
unit    "g"     # unit of emission
ry      1.0     # reference value (yearly)
rn      1.0     # reference value for deposition

########################### odorants ###########################
###                                                          ###
### The rated odorants must be specified directly after      ###
### [ODOR]. Adding or deleting rated odorants requires       ###
### adjustment of the program source code (TalInp.h,         ###
### TIP_ADDODOR = number or rated odorants).                 ###
###                                                          ###
################################################################

[ODOR]
unit   "OU"     # unit of emission
fc    100.0     # factor for odor hour
uc      "%"     # unit of odor hour
ry     10.0     # reference value (yearly)
dy        1     # number of decimals (yearly)

[ODOR_050]
unit   "OU"     # unit of emission
fc    100.0     # factor for odor hour
uc      "%"     # unit of odor hour
ry     10.0     # reference value (yearly)
dy        1     # number of decimals (yearly)

[ODOR_065]
unit   "OU"     # unit of emission
fc    100.0     # factor for odor hour
uc      "%"     # unit of odor hour
ry     10.0     # reference value (yearly)
dy        1     # number of decimals (yearly)

[ODOR_075]
unit   "OU"     # unit of emission
fc    100.0     # factor for odor hour
uc      "%"     # unit of odor hour
ry     10.0     # reference value (yearly)
dy        1     # number of decimals (yearly)

[ODOR_100]
unit   "OU"     # unit of emission
fc    100.0     # factor for odor hour
uc      "%"     # unit of odor hour
ry     10.0     # reference value (yearly)
dy        1     # number of decimals (yearly)

[ODOR_150]
unit   "OU"     # unit of emission
fc    100.0     # factor for odor hour
uc      "%"     # unit of odor hour
ry     10.0     # reference value (yearly)
dy        1     # number of decimals (yearly)

################################################################
